**Terms Last Revised: 6/06/2016**

**Z.1 Monitoring and Record keeping Requirements for the Fugitive Dust emissions from a Basic Oxygen Furnace (BOF) shop roof monitor**

* + - 1. The permittee shall perform visible emission readings of the fugitive emissions from the roof monitor serving the basic oxygen furnace (BOF) and shall maintain records of the readings. The visible emission readings shall be performed by certified readers in accordance with procedures contained in OAC rule 3745-17-03(B)(3). The observations shall include a minimum of four consecutive heats per week, balanced between the two BOFs over each calendar quarter, and shall be recorded on forms which have been approved by the Director (the appropriate District Office or local air agency). Therefore, for each calendar quarter, an approximately equal number of observations shall be performed for each of the BOFs. Observations shall commence when charging is initiated and shall end at the conclusion of the slagging operation.

**Z.2 Reporting Requirements for the Visible Emission readings for a BOF shop roof monitor**

* + - 1. Copies of the visible emission readings for the BOF shop roof monitor shall be submitted on a quarterly basis. The submissions shall occur by January 31, April 30, July 31, and October 31 of each year and shall include the readings performed during the previous calendar quarters.